{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Cills"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":18,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cills","index":0,"n_rows":66,"n_cols":8,"rows_kept":66,"cut":false,"hidden":false,"merged":[[44,0,44,7],[43,0,43,7],[65,0,65,7],[57,0,57,7],[58,0,58,7],[59,0,59,7],[60,0,60,7],[61,0,61,7],[62,0,62,7],[63,0,63,7],[64,0,64,7],[48,0,48,1],[50,0,50,1],[5,1,5,4],[6,1,6,4],[7,1,7,4],[8,0,8,7],[3,1,3,4],[5,5,5,7],[6,5,6,7],[7,5,7,7],[55,0,55,1],[49,0,49,1],[51,0,51,1],[54,0,54,1],[53,0,53,1],[52,0,52,1],[0,0,0,7],[3,5,3,7],[4,5,4,7],[4,1,4,4],[1,0,1,5],[2,6,2,7]]}
[]
["Cill Order Form"]
[null,null,null,null,null,null,"archital.co.uk"]
["Date ",null,null,null,null,"  Delivery Address "]
[" Name "]
["Company "]
["Order Reference "]
["Colour "]
[]
["Window","Type","Length ","A","B","C","D","Qty"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,{"$f":"SUM(H11:H42)","v":0}]
[]
["Lengths over 3m will be supplied in two sections with joining straps supplied free of charge"]
[]
[]
["Cill Types"]
["1. Standard with stopends"]
["2. Side Upstands"]
["3. Cut-out Side Upstands"]
["4. Full Plaster Stop"]
["5. Cut-out Plaster Stop"]
["6. Plain (no stop-ends)"]
["T. Trim"]
["C. Custom"]
[]
["Manufacturing Notes"]
["Our normal lead time is about 2 weeks."]
["Cills and pressings will be made using 2mm aluminium unless otherwise stated and are made to a \ntolerance of +/- 2mm. "]
["Items are made to the measurements provided. It is your responsibilty when providing measurements to allow for expansion of the aluminium."]
["Cills are painted on the outside only  - we can paint the underside on request for which there will be an additional charge."]
["Joins between side and rear upstands are not welded."]
["Coloured screws can be provided on request for a small charge."]
["Pressings longer than 3m will be supplied in two parts with a joining strap. "]
["Please check all items on delivery and advise us immediately of any issues."]